3/2/2025:

* Change the diodes. Footprint is tough to hand solder.
* Rotate the ESC/ TAB and 5 macro keys to reduce board dimension
* Add WS2812 leds.